* Turbine extractions are used as heat source in the process of air preheating.
* Low-temperature economizers are employed to absorb economizer outlet flue gas heat.
* Exergy analysis is carried out to find the effect of system optimization.
* The air preheat process’ heat transfer temperature difference is reduced.
* The novel system’s efficiency is increased under design and off-design conditions.